CPY Server Application – Firmware revisions

Document rev. 27/09/2022

|  |
| --- |
| Firmware release Rev.2.9.3 – 22080301 |
| |  |  | | --- | --- | | New features | * ID 6858 – ParkHelp Display management for Parkman Plant | | **Enhancements** | * ID 6877 – Improved login page visualization for low resolution monitors * ID 6850 – Digital Car Park: Added the setting of digital bay names * ID 6896 – CPY Server: The system info menu shows the MAC address with a wrong format | | **Bug fixing** | * ID 6805 – CPY Server: Alarm status was not shown when the bus generator modules disconnected from the Dupline network * ID 6862 – CPY Server: The display pop up didn’t appear in specific conditions | |

|  |
| --- |
| Firmware release Rev.2.8.3 – 22051702 |
| |  |  | | --- | --- | | New features |  | | **Enhancements** | * **ID 6854 – Cyber security: hardening of login authentication and input validation** | | **Bug fixing** | * ID 6792 – CPY Server: It was not possible to modify the BACnet configuration after having added new objects onto the CPY configuration * ID 6782 – CPY Server: It was not possible to generate “space statistics” reports over long time periods * ID 6862 – CPY Server: Pop-up display did not work as expected | |

|  |
| --- |
| Firmware release Rev.2.7.3 - 22021501 |
| |  |  | | --- | --- | | New features | * Generic digital input management via Smart Dupline® integration | | **Enhancements** | * ID 6764 - MAIA Cloud: MAIA Cloud client service watchdog hardened * ID 6771 - MAIA Cloud: Hardening of the VPN client service | | **Bug fixing** | - | |

|  |
| --- |
| Firmware release Rev.2.6.3 - 21121502 |
| |  |  | | --- | --- | | New features | * Maia Cloud compatibility | | **Enhancements** | - | | **Bug fixing** | * ID 6745 - Modem: Added support for Teltonika 4G USB modem * ID 6706 - WEBAPI: When change category to a bay the display showed a wrong counting value * ID 6699 - CP3App: Category setting for “Normal" status did not restore the "Green" LED colour in physical sensor * ID 6752 - FW upgrade via MAIA or HTTPS failed due to timeout | |

|  |
| --- |
| Firmware release Rev.2.5.3 - 21091701 |
| |  |  | | --- | --- | | New features | - | | **Enhancements** | - | | **Bug fixing** | * ID 6437 - CP3App: CP Map image did not upload on drawing window * ID 6646 - CP3App: "Exceeded MZC max value" error appeared while changing MZC values through API * ID 6686 - CP3App: Icons go back to default settings for display on "Drawing" after sending configuration to CPY server second time from UWP 3.0 Tool | |

|  |
| --- |
| Firmware release Rev.2.4.3 - 20102701 |
| |  |  | | --- | --- | | New features | - | | **Enhancements** | * ID 6256 – Added the possibility to change the category to indicators from scheduler | | **Bug fixing** | - | |

|  |
| --- |
| Firmware release Rev.2.3.3 - 20052801 |
| |  |  | | --- | --- | | New features | - | | **Enhancements** | * Cyber security: updated TLS certificate to version 1.3 * WEB API: Lanes and Lines are now filtered by the getGroups method | | **Bug fixing** | * BACnet configuration did not work properly * There was a missing translation during the firmware upgrade process | |

|  |
| --- |
| Firmware release Rev.2.2.3 - 20031301 |
| |  |  | | --- | --- | | New features | * Added Car monitoring functionality | | **Enhancements** |  | |

|  |
| --- |
| Firmware release Rev.2.1.3 - 20022701 |
| |  |  | | --- | --- | | New features | * Customizable locations tree | | **Enhancements** | * New icons for DISxRSE displays | |

|  |
| --- |
| Firmware release Rev.2.0.3 - 2019121301 |
| |  |  | | --- | --- | | New features | * Added support for the CP3 Outdoor solution | | **Enhancements** | * Added support for USB modem DIGICOM 4G USB (Huawei E909s-120) | | **Bug fixing** | * CPY Server did not start correctly after importing an old CPY database backup | |

|  |
| --- |
| Firmware release Rev.1.9.3 - 2019102201 |
| |  |  | | --- | --- | | New features | - | | **Enhancements** | * The configuration download to CPY has been improved * Faster loading of Park status view and Drawing view with many displays | | **Bug fixing** | * Displays are updated in a shorter time (the worst case requires 20 seconds) | |

|  |
| --- |
| Firmware release Rev.1.6.3 - 2019040501 |
| |  |  | | --- | --- | | New features | * Set offset to the displays | | **Enhancements** | * Added support for USB modem TeleOrigin RB900L (module Telit E910-EU V2) * For normal users, events of the sensors that last less than 30 seconds are hidden * Login timeout extended | |
| |  |  | | --- | --- | | Bug fixing | * Groups occupancy and daily aggregation of group occupancy data are not calculated * Changing the total available spaces in a MZC function is not updated before rebooting | |